For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove oil pan. Refer to Oil Pan Replacement.
2. Remove the cylinder head. Refer to Fuel Tank Replacement.

1 | Piston, Connection Rod, and Bearing Fastener (Qty: 8) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb ft)
2 | Piston, Connection Rod, and Bearing Connecting Rod (Qty: 4)
3 | Piston, Connection Rod, and Bearing