For 1990-2009 cars

## Front Seat Lumbar Support Replacement Driver/Passenger Seat Electric Lumbar

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove driver or passenger seat. Refer to Driver or Passenger Seat Replacement.
3. Remove the front seat back cushion pad. Refer to Front Seat Back Cushion Pad Replacement.

1 | Front Seat Lumbar Support Retainer (Qty: 10)

#### Procedure

1. Release the lumbar pump.
2. Disconnect the wiring harness connector from the lumbar pump.
3. Disconnect the wiring harness connector from the lumbar distributor.
4. Disconnect the wiring harness connector from the vent fan.
5. Cut cable straps.
6. Release the lumbar at backrest frame.
7. Remove lumbar assembly from backrest.

2 | Front Seat Lumbar Support

## Front Seat Lumbar Support Replacement Driver/Passenger Seat Manual Lumbar

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove driver or passenger seat. Refer to Driver or Passenger Seat Replacement.
3. Remove the front seat back cushion pad. Refer to Front Seat Back Cushion Pad Replacement.

1 | Front Seat Lumbar Support Retainer (Qty: 10)

#### Procedure

1. Release the lumbar pump.
2. Disconnect the wiring harness connector from the lumbar pump.
3. Disconnect the wiring harness connector from the lumbar distributor.
4. Disconnect the wiring harness connector from the vent fan.
5. Cut cable straps.
6. Release the lumbar at backrest frame.
7. Remove lumbar assembly from backrest.

2 | Front Seat Lumbar Support