For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the headlining trim panel. Refer to Headlining Trim Panel Replacement.

1 | Sunroof Housing Control Fastener (Qty: 12) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Disconnect wiring harness connector of sunroof motor.
2. Disconnect the water drain hoses in the front and rear.

Tip
For sunroof removal and installation it is necessary to have 2 technicians for support.

Tighten
9 N·m (80 lb in)

2 | Sunroof Housing