For 1990-2009 cars

## Windshield Washer Pump Replacement 68 HB

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse front liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Windshield Washer Pump

#### Procedure

1. Disconnect the windshield washer pump electrical connector.
2. Disconnect both windshield washer pump hoses from the washer pump.
3. Drain the windshield washer solvent container into a clean suitable container.
4. Using a small flat-bladed tool, remove the windshield washer pump seal from the windshield washer solvent container and inspect the seal, replace if damaged.

Tip
Using a small flat-bladed tool, remove the windshield washer pump from the windshield washer solvent container.