For 1990-2009 cars

## Charge Air Cooler Inlet Hose Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the engine shield. Refer to Engine Shield Replacement

1 | Charge Air Cooler Inlet Hose

## Charge Air Cooler Inlet Hose Replacement LBW/A28NET

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Turn the ignition OFF.
2. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
3. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
4. Remove the engine control module from the battery tray. Refer to NEED CELL LINK.

1 | Charge Air Cooler Inlet Hose Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
2 | Charge Air Cooler Inlet Hose Fastener Tighten X N·m (89 lb in)
3 | Charge Air Cooler Inlet Hose