For 1990-2009 cars

## Intake Manifold Disassemble LLU

1. Disconnect the evaporative emission pipe (1) from the intake manifold (3) and the evaporative emission pipe bracket (2).
2. Remove the evaporative emission pipe (1).
3. Remove the 2 fuel injection rail bolts (2).
4. Remove the fuel injection rail (3) from the intake manifold (1).
5. Remove the charger air bypass regulator solenoid vacuum valve bracket bolts (1).
6. Remove the charger air bypass regulator solenoid vacuum valve bracket (2) from the intake manifold (3).