For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the steering servo reservoir, refer to Power Steering Fluid Reservoir Replacement.

1 | Transmission Fluid Cooler Hose Cover
2 | Transmission Fluid Cooler Hose/ Pipe Quick-Connect Fitting Disconnection and Connection

#### Procedure

Mount the release tool round the pipe, press it in to the quick connector and turn for removal using DT-49662 disconnect tool .

#### Special Tools

DT-49662 Disconnect Tool 3/8"l

For equivalent regional tools, refer to Special Tools.