For 1990-2009 cars

#### Special Tools

• | EN 46106 Engine Flywheel Holding Tool

• | EN 45059 Torque Angle Sensor Kit

For equivalent regional tools, refer to Special Tools.

1. Install the automatic transmission flex plate (2).
2. Loosely install the NEW 8 automatic transmission flex plate bolts (1).
3. Install the EN 46106 holder .
4. Tighten the 8 automatic transmission flex plate bolts (1) to 30 N·m (22 lb ft).
5. Tighten the NEW 8 automatic transmission flex plate bolts an additional 45 degrees using the EN 45059 kit .
6. Remove the EN 46106 holder .