For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the passenger side instrument panel lower trim panel - passenger side. Refer to LINK.
3. Remove the instrument panel (I/P) lower extension side trim panel. Refer to Instrument Panel Lower Extension Side Trim Panel Replacement.

1 | Air Inlet Valve Actuator Fastener (Qty: 3)
2 | Air Inlet Valve Actuator

#### Procedure

Disconnect the air inlet valve actuator electrical connector.

Tip
Actuator is self-calibrating when connecting the battery.