For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove sunroof window. Refer to Sunroof Window Replacement.
2. Remove sunroof housing assembly.
3. Sunroof Window Height and Opening Fit Adjustment. Refer to Sunroof Window Height and Opening Fit Adjustment.

1 | Sunroof Housing Drain Gutter

#### Procedure

Clip the sunroof housing drain gutter out of bracket on the left and right side.