For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the exhaust front pipe. Refer to LINK.

1 | Transmission Rear Mount Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 62 N·m (45.7 lb ft)
2 | Transmission Rear Mount Fastener Tighten 100 N·m (73.8 lb ft)
3 | Transmission Rear Mount Fastener (Qty: 2) Tighten 110 N·m (81.1 lb ft)