For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement.
2. Remove the front side door window. Refer to Front Side Door Window Replacement.
3. Release the 2 window retainers, push the window to the full up position and tape in place.

1 | Front Side Door Window Regulator Fastener (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tip Use new fasteners. Tighten
9 N·m(80 lb in)

2 | Front Side Door Window Regulator Retainer

#### Procedure

Disconnect front side door window regulator electrical connector.

3 | Front Side Door Window Regulator