For 1990-2009 cars

Use the urethane adhesive for replacement of any urethane adhesive-installed window using the full cut method.

In the United States or Canada, you may use urethane adhesive systems which meet GM Specification GM 3651G:

Use these materials based on specific manufacturer. Do NOT intermix primers or adhesives from one manufacturer to another.

Always follow the system manufacturer's instructions for application, handling, and curing.