For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the engine shield. Refer to Engine Shield Replacement.

1 | Oil Pan Drain Plug Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Drain the oil from the vehicle.

Tighten
25 N·m(18 lb ft)

2 | Oil Filter Cover

#### Procedure

1. Release the oil filter cover and allow the oil in the oil filter housing to drain using EN-49377 retainer .
2. Install new oil filter cover seals.

Tighten
25 N·m (18 lb ft)

#### Special Tools

EN-49377 Oil Retainer

For equivalent regional tools, refer to Special Tools.

3 | Oil Filter Tip After repairs, for engine oil specifications refer to Engine Mechanical Specifications.