For 1990-2009 cars

Note: Ensure that the crankshaft is in the stage one timing drive assembly position.

1. Install the primary timing chain (1).
2. Wrap the primary timing chain around the large sprockets of each timing chain idler sprocket and the crankshaft sprocket.
3. The timing chain idler sprocket bank 2 timing mark (1) will align with a primary timing chain link (2).
4. The crankshaft sprocket timing mark (2) will align with a primary timing chain link (1).
5. The timing chain idler sprocket bank 1 timing mark (2) will align with a primary timing chain link (1).
6. Ensure all the timing marks (2, 3, 6) are properly aligned with the primary timing chain links (1, 4, 5).