For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the liftgate trim finish panel. Refer to LINK.
2. Use a suitable tool to detach the left and right corner of the rear end spoiler.
3. From the rear to the end spoiler fascia, apply a double layer of masking tape around the perimeter of the painted surfaces.

1 | Rear End Spoiler Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
2 | Rear End Spoiler