For 1990-2009 cars

## Charge Air Cooler Outlet Hose Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the engine shield. Refer to Engine Shield Replacement.

1 | Charge Air Cooler Outlet Hose

## Charge Air Cooler Outlet Hose Replacement LBW/A28NET

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Turn the ignition OFF.
2. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
3. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
4. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.
5. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Charge Air Cooler Outlet Hose Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
2 | Charge Air Cooler Outlet Hose Fastener (Qty: 3) Tighten 9 N·m (80 lb in)
3 | Charge Air Cooler Outlet Hose