For 1990-2009 cars

## Front Seat Adjuster Motor Replacement Driver or Passenger Seat 8-Way Power

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove driver or passenger seat. Refer to Driver or Passenger Seat Replacement.

1 | Front Seat Adjuster Motor Fastener (Qty: 2)

#### Procedure

1. Remove the seat adjuster motor out of the both brackets at seat frame.
2. Remove the seat adjuster motor cables by pulling the cables out of adjuster.
3. Disconnect the electric connector.