For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove rear compartment lid inner panel trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement.

1 | Rear Compartment Lid Outside Handle Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Compartment Lid Outside Handle

#### Procedure

1. Disconnect the electrical connector.
2. Transfer components as necessary.