For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

If equipped, remove the fuel tank protector. Refer to Fuel Tank Protector Replacement.

Warning: Gasoline or gasoline vapors are highly flammable. A fire could occur if an ignition source is present. Never drain or store gasoline or diesel fuel in an open container, due to the possibility of fire or explosion. Have a dry chemical (Class B) fire extinguisher nearby.

1 | Fuel Filter Assembly Cover Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Release the fuel filter assembly fastener using a spanner.
2. Remove the fuel filter assembly cover.

2 | Fuel Filter Retaining Cover

#### Procedure

1. Release the fuel filter retaining cover retainers by pulling downwards.
2. Remove the fuel filter retaining cover.

3 | Fuel Filter Caution: Do not use a screwdriver or punch to remove the seal. Using a screwdriver or punch to remove the seal may damage the aluminum housing sealing surface.