For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the battery tray, refer to Battery Tray Replacement.
2. Remove the shift control from the transmission control, refer to Transmission Control Replacement.

1 | Range Selector Lever Cable

#### Procedure

1. Remove the shift control cable seal from the bulkhead.
2. Remove the cable from the clip.
3. Remove the shift control cable from the lever.
4. Adjust the shift control cables. Refer to Range Selector Lever Cable Adjustment.