For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear axle assembly. Refer to Rear Axle Replacement.

1 | Limited Slip Differential Clutch Pipe (Qty: 2) Warning: The hydraulic pressure in the differential clutch is very high. To prevent personal injury, wait for at least 10 minutes before removing any parts from the differential clutch.

#### Procedure

Fit tool DT-49132 removal tool to the quick-release coupling, turn slightly and pull out the pipe.

#### Special Tools

DT-49132 Removal Tool

For equivalent regional tools, refer to Special Tools.