For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the engine cover. Refer to Engine Cover Replacement
2. Remove the battery negative terminal. Refer to Battery Negative Cable Disconnection and Connection
3. Release the electrical connector.

Warning: Gasoline or gasoline vapors are highly flammable. A fire could occur if an ignition source is present. Never drain or store gasoline or diesel fuel in an open container, due to the possibility of fire or explosion. Have a dry chemical (Class B) fire extinguisher nearby.

1 | Fuel Injector Fuel Rail Assembly Inlet and Outlet Pipe Fasteners (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m 18 lb ft
2 | Fuel Injection Fuel Rail Pressure Sensor
3 | Fuel Injector Fuel Rail Assembly Fasteners (Qty: 3) Tighten 22 N·m 16 lb ft
4 | Fuel Injector Fuel Rail Assembly