For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Front Bumper Fascia Center Support Bracket Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Front Bumper Fascia Center Support Bracket Retainer (Qty: 2)
3 | Front Bumper Fascia Center Support Bracket