For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Release electric park brake.

1.1. | Set ignition in Run mode and put your foot on top of the service brake.

1.2. | Press park brake switch down and hold for 5 seconds, then a solid yellow telltale is shown on instrument panel.

1.3. | Press park brake switch again within 5 seconds, then a flashing yellow telltale is shown on instrument panel.

2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
3. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
4. Remove the rear wheelhouse panel liner. Refer to Rear Wheelhouse Panel Liner Replacement .

1 | Electric Park Brake Module Cable
2 | Electric Park Brake Module Clips (Qty: 2)
3 | Electric Park Brake Module Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 9.5 N·m (84 lb in)
4 | Electric Park Brake Module

#### Procedure

Program the electric park brake module. Refer to Electronic Parking Brake Control Module Programming and Setup .