For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. SIR disabling and enabling. Refer to SIR Disabling and Enabling.
2. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
3. Remove driver or passenger seat replacement. Refer to Driver or Passenger Seat Replacement.

1 | Driver Seat Belt Buckle Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 45 N·m (33 lb ft)
2 | Driver Seat Belt Buckle

#### Procedure

Disconnect electrical connector.