For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Safety Glasses Warning in the Preface section.

#### Preliminary Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.

Caution: In order to avoid oil pan damage and possible engine failure, insert a block of wood that spans the width of the oil pan bottom between the oil pan and the jack support.

2. Remove the engine shield. Refer to Engine Shield Replacement.
3. Remove the front wheelhouse rear liner. Refer to Front Wheelhouse Rear Liner Replacement.
4. Remove the battery tray. Refer to Battery Tray Replacement.
5. Remove the transmission mount bracket. Refer to Transmission Mount Bracket Replacement - Left Side.

1 | Transmission Mount