For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the driver or passenger seat. Refer to Driver or Passenger Seat Replacement.
3. Remove the front seat back cushion pad. Refer to LINK 15604.

1 | Rivet (Qty: 4)

#### Procedure

1. Drill out rivet at front seat head restraint actuator.
2. Remove front seat head restraint actuator from backrest frame.
3. Position front seat head restraint actuator at backrest frame.
4. Rivet with caliper.

Tip
Use only original rivets!

2 | Front Seat Head Restraint Actuator