For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Side Door Upper Hinge to Body Fastener (Upper) (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Support the door before removing the hinge fastener.
2. Disconnect the door electrical connector.

Tighten:
22 N·m (16 lb ft).

2 | Rear Side Door Upper Hinge to Door Fastener (Upper) (Qty: 2) Tighten 22 N·m (16 lb ft).
3 | Rear Side Door Upper Hinge

#### Procedure

Check the door for proper alignment, adjust as necessary.

4 | Rear Side Door Lower Hinge to Body Fastener (Lower) (Qty: 2) Tighten 22 N·m (16 lb ft).
5 | Rear Side Door Lower Hinge to Door Fastener (Lower) (Qty: 2) Tighten 22 N·m (16 lb ft).
6 | Rear Side Door Lower Hinge

#### Procedure

Check the door for proper alignment, adjust as necessary.