For 1990-2009 cars

## Rear Spring Replacement GNC

Callout | Component Name
--- | ---
Warning: To prevent personal injury and/or component damage, use the proper tools to support the lower control arm when removing the coil spring. The coil spring is under extreme pressure and can become a projectile should the spring separate from the lower control arm before all of the tension is relieved.

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear tire and wheel. Refer to Tire and Wheel Removal and Installation.

1 | Rear Axle Lower Control Arm Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Install NEW bolt.

Tighten
70 N·m(51 lb ft) + 90 degrees + 15 degrees

2 | Rear Spring

#### Procedure

1. Using a suitable jack stand, support the knuckle.
2. Using a adjustable jack stand, slowly lower control arm downward.
3. Remove the coil spring from the lower control arm.
4. If needed, remove the rear spring upper insulator or the lower spring insulator.

## Rear Spring Replacement GNE

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove and support the brake calliper, without disconnecting the hydraulic brake hose from the caliper. Refer to Rear Brake Caliper Replacement.
4. Losen the stabilizer shaft. Refer to Stabilizer Shaft Link Replacement.

1 | Rear Spring

#### Procedure

Use CH-49671 compressor to compress the spring.

#### Special Tools

CH-49671 Spring Compressor

For equivalent regional tools. Refer to Special Tools.