For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear side door window outer sealing strip. Refer to Rear Side Door Window Outer Sealing Strip Replacement.
2. Release the rear side door water deflector, if necessary. Refer to Rear Side Door Water Deflector Replacement.

1 | Rear Side Door Window Rear Channel Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Rear Side Door Window Rear Channel