For 1990-2009 cars

## Engine Coolant Thermostat Housing Replacement LBW/A28NET

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the catalytic converter. Refer to Catalytic Converter Replacement.

1 | Heater Outlet Pipe Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 62 N·m (46 lb ft)
2 | Heater Outlet Pipe Tip Do NOT remove the heater outlet pipe from the vehicle. Install a NEW O-ring.
3 | Radiator Outlet Pipe Tip Do NOT remove the radiator outlet pipe from the vehicle. Install a NEW O-ring.
4 | Engine Coolant Thermostat Housing

#### Procedure

1. Remove the engine coolant thermostat housing. Refer to Engine Coolant Thermostat Housing Removal.
2. Install the engine coolant thermostat housing. Refer to Engine Coolant Thermostat Housing Installation.

## Engine Coolant Thermostat Housing Replacement LDK/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle by its full height. Refer to Lifting and Jacking the Vehicle.
2. Draing the cooling system. Refer to Cooling System Draining and Filling.
3. Remove the engine coolant temperature sensor. Refer to Engine Coolant Temperature Sensor Replacement.
4. Release the radiator outlet hose. Refer to Radiator Outlet Hose Replacement.
5. Release the radiator surge tank engine hose. Refer to XXX.
6. Release the heater outlet hose. Refer to Heater Outlet Hose Replacement.
7. Release the heater inlet hose. Refer to XXX.
8. Release the turbocharger coolant return pipe. Refer to XXX.

1 | Engine Coolant Thermostat Housing Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb ft)
2 | Engine Coolant Thermostat Housing