For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the battery tray. Refer to Battery Tray Replacement.
2. Remove the lever linkage. Refer to TBD.
3. Disconnect the TCM electrical connector.

1 | Transmission Control Module Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Transmission Control Module

#### Procedure

1. Set the inner, rotating section of the control module so that the arrow is pointing towards the marking on the housing.
2. Carry out adaptation, resetting. Refer to Transmission Adaptive Functions.
3. Program the gear selector position sensor in neutral, using the scan tool.

Tip
Twisting or tilting of the transmission control module electrical connector while disconnecting may result in bent or misaligned electrical terminal pins.