For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front wheelhouse front liner to access the bulb. Refer to Front Wheelhouse Front Liner Replacement.
2. Disconnect the forward lamp electrical harness connector from the fog lamp bulb socket.

1 | Front Fog Lamp Projector Bulb

#### Procedure

Twist the bulb socket counterclockwise to remove from the lamp housing.