For 1990-2009 cars

#### Special Tools

• | EN 45059 Torque Angle Sensor Kit

• | EN 46792 Crankshaft/Flywheel Holder

For equivalent regional tools, refer to Special Tools.

1. Install the flywheel.
2. Install the 6 NEW flywheel bolts.

Caution: Refer to Fastener Caution in the Preface section.

3. Hold the crankshaft with EN 46792 holder , tighten the bolts in sequence evenly to 160 N·m(118 lb ft) , using the EN 45059 angle sensor .