For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear window wiper arm. Refer to Rear Window Wiper Arm Replacement.
2. Remove the liftgate trim finish panel. Refer to Liftgate Trim Finish Panel Replacement.

1 | Rear Window Wiper Motor Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 3.5 N·m (31 lb in)
2 | Rear Window Wiper Motor