For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Side Door Upper Hinge to Body Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Support the door before removing the hinge fastener.
2. Disconnect the door electrical connector.

Tighten
22 N·m (16.2 lb ft)

2 | Front Side Door Upper Hinge to Door Fastener (Qty: 2) Tighten 22 N·m (16.2 lb ft)
3 | Front Side Door Upper Hinge
4 | Front Side Door Lower Hinge to Body Fastener (Qty: 2) Tighten 22 N·m (16.2 lb ft)
5 | Front Side Door Lower Hinge to Door Fastener (Qty: 2) Tighten 22 N·m (16.2 lb ft)
6 | Front Side Door Lower Hinge