For 1990-2009 cars

## Rear Spring, Insulator, and Jounce Bumper Replacement GNE

Callout | Component Name
--- | ---
Warning: To prevent personal injury and/or component damage, use the proper tools to support the lower control arm when removing the coil spring. The coil spring is under extreme pressure and can become a projectile should the spring separate from the lower control arm before all of the tension is relieved.

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the rear spring. Refer to Rear Spring Replacement.

1 | Coil Spring Insulators

## Rear Spring, Insulator, and Jounce Bumper Replacement GNC

Callout | Component Name
--- | ---
Warning: To prevent personal injury and/or component damage, use the proper tools to support the lower control arm when removing the coil spring. The coil spring is under extreme pressure and can become a projectile should the spring separate from the lower control arm before all of the tension is relieved.

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the rear spring. Refer to Rear Spring Replacement.

1 | Coil Spring Insulators