For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: In order to avoid oil pan damage and possible engine failure, insert a block of wood that spans the width of the oil pan bottom between the oil pan and the jack support.

#### Preliminary Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
2. Remove the engine shield. Refer to Engine Shield Replacement.
3. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Engine Mount Fastener (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten 58 N·m(43 lb ft)
2 | Engine Mount - Right Side Fastener Tighten 63 N·m(46 lb ft)
3 | Engine Mount - Right Side