For 1990-2009 cars

## Intake Manifold Assemble LLU

1. Install the charger air bypass regulator solenoid valve bracket (2) to the intake manifold (3).
2. Install the charger air bypass regulator solenoid valve bracket bolts (1) and tighten to 8 N·m (71 lb in).
3. Install the fuel injection rail (3) to the intake manifold (1).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the 2 fuel injection rail bolts (2) and tighten to 8 N·m (71 lb in).
5. Connect the evaporative emission pipe (1) to the evaporative emission pipe bracket (2) and the intake manifold (3).