For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the engine shield. Refer to Engine Shield Replacement.

1 | Resonator Rear Securing Fastener (Qty: 3) Caution: The exhaust temperature sensor and exhaust pressure differential sensor line fittings may be difficult to remove when the engine exhaust system temperature is below 48°C (120°F). Excessive force may damage the threads in the exhaust manifold or exhaust pipe.

Caution: Refer to Fastener Caution in the Preface section.

Tighten
23 N·m (17 lb ft)

2 | Resonator Front Securing Fastener (Qty: 3) Tighten 23 N·m (17 lb ft)
3 | Resonator Rubber Mounting Fastener (Qty: 2)

#### Procedure

Disconnect the resonator rubber retainers.

4 | Resonator

#### Procedure

Replace resonator gaskets front and rear.