For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the Rear Compartment Lid Inner Panel Trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement.

1 | High Mount Stop Lamp Fastener (Qty: 4)
2 | High Mount Stop Lamp

#### Procedure

1. Disconnect the electrical connector at the high mount stop lamp.
2. Use a small flat-bladed tool to release the high mount stop lamp locking retainer starting at the left or right side of the lid compartment.
3. Use new seal.
4. Hand tighten only, no torque required.