For 1990-2009 cars

## Camshaft Replacement Exhaust

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the Camshaft Exhaust Sprocket. Refer to LINK.
2. Remove the camshaft front bridge. Refer to LINK.

1 | Exhaust Camshaft Fastener (Qty: 8) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb ft)
2 | Exhaust Camshaft Bridge (Qty: 4)
3 | Exhaust Camshaft

## Camshaft Replacement Intake

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the Camshaft Intake Sprocket. Refer to LINK.
2. Remove the camshaft front bridge. Refer to LINK.

1 | Intake Camshaft Fastener (Qty: 8) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb ft)
2 | Intake Camshaft Bridge (Qty: 4)
3 | Intake Camshaft