For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front bumper in order to access the locking tabs on the radiator grille assembly. Refer to Front Bumper Fascia Replacement.
2. Remove the front bumper fascia energy upper absorber. Refer to Front Bumper Fascia Energy Upper Absorber Replacement.

1 | Radiator Grille

#### Procedure

Release the 18 locking front bumper tabs securing the radiator grille to the front bumper.