For 1990-2009 cars

## Engine Oil Cooler Housing Installation LLU

1. Clean the engine oil cooler housing to engine block sealing surfaces.
2. Install NEW gaskets.
3. Install the engine oil cooler inlet pipe (3).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the engine oil cooler housing (1) and the 5 engine oil cooler housing bolts (2) and tighten to 25 N·m (19 lb ft).
5. Install the thermostat housing coolant pipe (2) to the engine oil cooler housing.
6. Install the 2 thermostat housing coolant pipe bolts (1) and tighten to 8 N·m (71 lb in).