For 1990-2009 cars

## Exhaust Heat Shield Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the exhaust manifold heat shield. Refer to Exhaust Manifold Heat Shield Replacement
2. Remove position 1 exhaust temperature sensor. Refer to Exhaust Temperature Sensor Replacement - Position 1
3. Remove heated oxygen sensor 1. Refer to Heated Oxygen Sensor 1 Replacement

1 | Exhaust Heat Shield Fastener (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m(77 lb in)
2 | Exhaust Heat Shield

## Exhaust Heat Shield Replacement LDE/A16XER, 2H0/A18XER

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the exhaust system. Refer to Exhaust System Replacement.

1 | Front Exhaust Heat Shield Fastener (Qty: 8) Caution: Refer to Fastener Caution in the Preface section. Tighten 1,5N·m (13 lb in)
2 | Exhaust Heat Shield