For 1990-2009 cars

## Engine Oil Cooler Installation LDK

Note: The oil cooler cannot be flushed or otherwise cleaned of contamination. Replace the oil cooler if a mechanical condition is suspected that could cause the oil cooler to be contaminated.

1. Install the oil cooler (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the oil cooler bolts (2) and tighten to 25 N·m (18 lb ft).