For 1990-2009 cars

1. Install the positive crankcase ventilation oil separator (3).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the positive crankcase ventilation oil separator bolts (1, 5) and tighten to XX N·m (XX lb ft).
3. Connect the quick connect fitting from the oil separator hose (4) to oil pan.
4. Install the positive crankcase ventilation oil separator hose.
5. Install the positive crankcase ventilation oil separator hose clamp (2).