For 1990-2009 cars

## Air Conditioning Compressor and Condenser Hose Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging
2. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement
3. Remove the charge air inlet hose. Refer to Charge Air Cooler Inlet Pipe and Outlet Pipe Replacement
4. Remove the right headlamp. Refer to Headlamp Replacement

1 | Compressor and Condenser Hose Fasteners (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 22 N·m(16 lb ft)
2 | Air Conditioning Compressor and Condenser Hose Use new sealing washer. Refer to Sealing Washer Replacement

## Air Conditioning Compressor and Condenser Hose Replacement A20NHT/LDK

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the front bumper fascia assembly. Refer to Front Bumper Fascia Replacement.

1 | A/C Compressor and Condenser Hose Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Remove the A/C compressor and condenser hose from the A/C evaporator hose and cap hose.

Tighten
20 N·m (15 lb ft)

2 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

3 | A/C Compressor Hose Fastener

#### Procedure

Remove the A/C compressor hose from the A/C compressor and cap hose.

Tighten
22 N·m (15 lb ft)

4 | Sealing Washer

#### Procedure

Remove and discard sealing washers. Refer to Sealing Washer Replacement.

5 | A/C Condenser Hose Fastener Tighten 20 N·m (15 lb ft)
6 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

7 | A/C Compressor and Condenser Hose Assembly

## Air Conditioning Compressor and Condenser Hose Replacement LWB/A28NET

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the front bumper fascia assembly. Refer to Front Bumper Fascia Replacement.
3. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.

1 | A/C Compressor and Condenser Hose Fastener Caution: Refer to Fastener Caution in the Preface section. Tip Remove the A/C compressor and condenser hose from the A/C evaporator hose and cap hose. Tighten
20 N·m (15 lb ft)

2 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

3 | A/C Compressor Hose Fastener

#### Procedure

Remove the A/C compressor hose from the A/C compressor and cap hose.

Tighten
20 N·m (15 lb ft)

4 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

5 | A/C Condenser Hose Fastener Tighten 20 N·m (15 lb ft)
6 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

7 | A/C Compressor and Condenser Hose Assembly

## Air Conditioning Compressor and Condenser Hose Replacement LDE/A16XER, 2H0/A18XER

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the front bumper fascia assembly. Refer to Front Bumper Fascia Replacement.

1 | A/C Compressor and Condenser Hose Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Remove the A/C compressor and condenser hose from the A/C evaporator hose and cap hose.

Tighten
22 N·m (15 lb ft)

2 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

3 | A/C Compressor Hose Fastener

#### Procedure

Remove the A/C compressor hose from the A/C compressor and cap hose.

Tighten
20 N·m (15 lb ft)

4 | Sealing Washer

#### Procedure

Remove and discard sealing washers. Refer to Sealing Washer Replacement.

5 | A/C Condenser Hose Fastener Tighten 20 N·m (15 lb ft)
6 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

7 | A/C Compressor and Condenser Hose Assembly