For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the sunroof housing assembly. Refer to Sunroof Module Assembly Replacement.
2. Remove the sunroof sunshade motor. Refer to Sunroof Sunshade Motor Replacement.
3. Remove the sunroof housing drain gutter. Refer to Sunroof Housing Drain Gutter Replacement.
4. Remove the sunroof sunshade. Refer to Sunroof Sunshade Replacement.

1 | Sunroof Panel/Window Guide

#### Procedure

1. Remove the two rear sunroof module assembly brackets.
2. Move the sunroof panel/window guide left side and right side rearward out of the sliding rail.
3. After installation adjust sunroof module.
4. After the installation adjust the sunroof sunshade motor.
5. After the installation adjust the sunroof window.
6. Functional check sunroof.
7. Visual check sunroof.